Specifying the STC Box SealTM

August 10, 2018

The Box Seal can be specified in either Section 078413 “Penetration Firestopping” under Fill Materials, or in Section 262726 “Wiring Devices” with Wall Plates.

Wall Plate Gaskets: “Box Seal” by STC Sound Control.

1. Manufacturer's standard molded neoprene formed to fit the electrical device and wall plate and in accordance with ASTM C 919.
2. Sound Rating: Increases STC of recessed outlets by 7 dBA or higher according to ASTM E90 (small scale).
3. Fire Rating: Single duplex configuration UL-listed as a Wall Opening Protective Device for use in 1-hour fire-rated walls, including back-to-back outlets.